## Phidget Power Guard.lvlib:PowerGuardSetFanMode.vi

The `FanMode` dictates the operating condition of the fan.

- Choose between on, off, or automatic (based on temperature).
- If the `FanMode` is set to automatic, the fan will turn on when the temperature reaches 70°C and it will remain on until the temperature falls below 55°C.
- If the `FanMode` is off, the device will still turn on the fan if the temperature reaches 85°C and it will remain on until it falls below 70°C.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Fan Mode The fan mode value
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
SAF1000_0 v101 v102 | SAF1000_0 v110 v120
FAN_MODE_OFF | 1 | ✓ | ✓
FAN_MODE_ON | 2 | ✓ | ✓
FAN_MODE_AUTO | 3 | ✓ | ✓
SAF1000_0 (ver: 101, 102) Power Supply Protector: Def: FAN_MODE_AUTO SAF1000_0 (ver: 110, 120) Power Supply Protector: Def: FAN_MODE_AUTO

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.