## Phidget Power Guard.lvlib:PowerGuardSetPowerEnabled.vi

When `PowerEnabled` is true, the device will connect the input to the output and begin monitoring.

- The output voltage is constantly monitored and will be automatically disconnected from the input when the output exceeds the `OverVoltage` value.
- `PowerEnabled` allows the device to operate as a Solid State Relay, powering on or off all devices connected to the output.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Power Enabled The power enabled value. SAF1000_0 (ver: 101, 102) Power Supply Protector: Def: 0 SAF1000_0 (ver: 110, 120) Power Supply Protector: Def: 0

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.