## Phidget Motor Velocity Controller.lvlib:MotorVelocityControllerSetInductance.vi

The controller will attempt to measure the inductance of your motor when opened. This value is used to improve control of the motor.

- Set this value during the `Phidget_Attach` event to skip motor characterization (including the audible beeps). You can use a previously saved `MotorVelocityControllerInductance` value, or information from your motor's datasheet.

For more information about `MotorVelocityControllerInductance`, visit our MotorVelocityController API Guide

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Inductance The inductance of your motor Units: henries (H) DCC1020_0 (ver: 103) Velocity Controller: Min: 0.0001 Max: 0.01 DCC1120_0 (ver: 104) Velocity Controller: Min: 0.0001 Max: 0.01

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.