## Phidget Temperature Sensor.lvlib:TemperatureSetRTDType.vi

The `TemperatureSensorRTDType` must correspond to the RTD type you are using in your application.

- If you are unsure which `TemperatureSensorRTDType` to use, visit your device's User Guide for more information.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| RTD Type The RTD type
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
TMP1200_0 v104 v105 v106 v107 v108 v109 v110 | TMP1200_1 v300 v301 v302 | TMP1202_0 v100
RTD_TYPE_PT100_3850 | 1 | ✓ | ✓ | ✓
RTD_TYPE_PT1000_3850 | 2 | ✓ | ✓ | ✓
RTD_TYPE_PT100_3920 | 3 | ✓ | ✓ | ✓
RTD_TYPE_PT1000_3920 | 4 | ✓ | ✓ | ✓
TMP1200_0 (ver: 104, 105, 106, 107, 108, 109, 110) RTD input: Default: RTD_TYPE_PT1000_3850 TMP1200_1 (ver: 300, 301, 302) RTD input: Default: RTD_TYPE_PT1000_3850 TMP1202_0 (ver: 100) RTD input: Default: RTD_TYPE_PT1000_3850

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.